Updates history


210601 Release
Suits:
---* QA03-SDA-DIS-VAC-XXX-XXX with external UDT, or QA03-SDA-DIS-VAC-XXX-UDT
---* also for IOM, TMT
---* not for dual probes
Mind this:
Changes:
New:
---* The screen brightness is added to the crossmeter at the bottom, as a value 0..16
---* The SN of the TMT and TMP can be added to the system information
Removed:

210518a Temporary release
Suits:
---* QA03-SDA-DIS-VAC-XXX-XXX with external UDT, or QA03-SDA-DIS-VAC-XXX-UDT
---* also for IOM, TMT
---* not for dual probes
Mind this:
---* Enter or check the Solids density again and save.
Changes:
---* The flow meter can work on it self, UDT can be disconnected
---* PID controller improved
---* Minor changes and corrections
---* Short link to Offline Mode in Arenal Factory Menu
---* Saving data is not protected by confirm, not save and cancel
New:
---* Volume flow totalizer added
Removed:
---* 


210107 Temporary release
Suits:
---* QA03-SDA-DIS-VAC-XXX-XXX with external UDT, or QA03-SDA-DIS-VAC-XXX-UDT
---* also for IOM, TMT
---* not for dual probes
Mind this:
---* Enter the Solids density again and save.
Changes:
---* The Density of Solids is saved in another database. Therefor, from this version, the user needs to enter this value again and save.
---* The calculation of the production tonnage of slurry and solids is updated.
---* The HMI is working on a faster rate than 1 seconds. Timed calculations (like production) are corrected for this.
New:
---* In User Settings, page 2, the user can select if the production is reset at 00:00 or not. A green light will appear if this is set. Red will deactivate this function. In any time the user can press the button ResetProduction
Removed:
---* 

20191113 Release Slurry Mass flow Analyser
Suits:
---* QA03-SDA-DIS-VAC-XXX-XXX with external UDT, or QA03-SDA-DIS-VAC-XXX-UDT
---* also for IOM, TMT
---* not for dual probes
Mind this:
---* IOM and TMT work individually in the new software. For each unit connected
     you need to connect it also by software. Go to Configuration Menu, select the transmitter 
     or module to be connected, go to Modbus RTU and turn on the unit.
Changes:
---* SG and density calibrations are now integrated into one calibration. Calibrating one will also calibrate the other.
     Please note that if you calibrated on density, you should transfer those values to SG calibration before updating.
---* Totalizers for slurry / solids production do not reset upon restart.
---* The unit (m/s or m3/h) can now be selected for flow mA out.
---* The number of significant digits for several measurement values.
New:
---* Software for our Attenuation measurement system, for specific application that uses two probes on both sides of a pipe.
---* End results can be read from TCPIP register. See manual for details.
Removed:
---* Weight balance scale transmitter


20190723 Release Slurry Mass flow Analyser
Suits:
---* QA03-SDA-DIS-VAC-XXX-XXX with external UDT, or QA03-SDA-DIS-VAC-XXX-UDT
---* also for IOM, TMT (early release)
---* not for dual probes
Mind this:
---* IOM and TMT work individually in the new software. For each unit connected
     you need to connect it also by software. Go to Configuration Menu, select the transmitter 
     or module to be connected, go to Modbus RTU and turn on the unit.
Corrections:
---* minor screen updates
---* Improvement of Slurry Type Calibration. Each slurry has it own thermal-physical characteristic which now can be 
     implemented. The function is visible during temperature changes. After the implementation, log the data for one-two weeks,
     send the data of the usb stick to Arenal and you get further instructions to change some parameters.
New:
---* First implementation of the weight balance scale transmitter. This software is not yet fully operational;

Version B:
---* Fixed a bug which made it impossible to select m3/h for flow mA in.
Version C:
---* Added extra features for early release for thermal massflow transmitter.
Version D:
---* Fixed a bug which resulted in an incorrect TSS reading.


20190503 (intermediate release)
Suits:
---* QA03-SDA-DIS-VAC-XXX-XXX with external UDT, or QA03-SDA-DIS-VAC-XXX-UDT
---* also for IOM, TMT
---* not for dual probes
Mind this:
---* IOM and TMT work individually in the new software. For each unit connected
     you need to connect it also by software. Go to Configuration Menu, select the transmitter 
     or module to be connected, go to Modbus RTU and turn on the unit.
Corrections:
---* increase in operational log functions
---* auto-reminder for watercalibration for dredgers, screen update
---* remote sampling (taking a sample for laboratory) by external digital input I3
New:
---* Temperature dependent SG calibration introduced. In case a temperature effect appears to be visable,
     small effects can be updated in the software. This requires assistance from Arenal during the temperature behaviour
     and the correction in the analyser. In later software, after an evaluation period, this will automatised.
---* Starting up without USB stick or with failing USB stick, is now possible. After a software update however, the USB
     stick is needed to upload the settings and calibration file in the memory.


20190429c (partially released 7/5/2019)
Suits:
---* QA03-SDA-DIS-VAC-XXX-XXX with external UDT, or QA03-SDA-DIS-VAC-XXX-UDT
---* also for IOM, TMT
---* not for dual probes
Mind this:
---* IOM and TMT work individually in the new software. For each unit connected
     you need to connect it also by software. Go to Configuration Menu, select the transmitter 
     or module to be connected, go to Modbus RTU and turn on the unit.
Corrections:
---* corrections in flow measurement, TMT
---* displays corrected for massflow and solids production
New:
---* remote sampling (taking a sample for laboratory) by external digital input I3
---* auto-reminder for watercalibration for dredgers


20190304a (not released)
Suits:
---* QA03-SDA-DIS-VAC-XXX-XXX with external UDT, or QA03-SDA-DIS-VAC-XXX-UDT
---* not for IOM, TMT
---* not for dual probes
- Correction of solids density unit from ton/m3 to kg/m3
- span possibility added on mA-in-3.

20190226 (released)
Suits:
---* QA03-SDA-DIS-VAC-XXX-XXX with external UDT, or QA03-SDA-DIS-VAC-XXX-UDT
---* not for IOM, TMT
---* not for dual probes
- Correction in the polynomial 3 selection software. All software versions from 190118 require update.
  The polynomial 3 is not selected: instead number 4 is selected, which means that the value is inaccurate.

20190222
Suits:
---* QA03-SDA-DIS-VAC-XXX-XXX with external UDT, or QA03-SDA-DIS-VAC-XXX-UDT
---* not for IOM, TMT
---* not for dual probes
- A popup is made for the jpg capture of the screen to show the user the file number of the next jpg.
  User can change the number. By pressing "File No:" the popup removes from the screen.
- Operational Log extended with to more inputs

20190219
Suits:
---* QA03-SDA-DIS-VAC-XXX-XXX with external UDT, or QA03-SDA-DIS-VAC-XXX-UDT
---* not for IOM, TMT
---* not for dual probes
- The ProFace 5.7"is made similar equal to the dredging unit (7"), which means that the production results per shift is calculated.
- For the production of solids tonnes/h, a pulse output on digital_output_4 is available. As soon as a new ton is produced a pulse is given.
  The shift needs to be (re)started after every software update. Setting is retentative.
- Correction of the logging files, which does not work properly after the first file is full: it did not start up a new file.

20190204
Suits:
---* QA03-SDA-DIS-VAC-XXX-XXX with external UDT or QA03-SDA-DIS-VAC-XXX-UDT
---* not for IOM, TMT
---* not for dual probes
- TOF offset now adjustable per 0,1 ns
- Alarm added when TOF is under minimum value of the calibration range
- Improved air/water calibration. Is moved to the field calibration.
- A three point calibration has been added
- A cross meter was added for dredging applications
- Added the variable Slurry Production and SolidsProduction.
- Added the logging information for creating dredging reports (SAMPL03)



